SECTION 09 80 00

ACOUSTIC ROOM COMPONENTS

Display hidden notes to specifier. (Don't know how? [Click Here](https://www.arcat.com/sd/display_hidden_notes.shtml))

*Copyright 2022 - 2023 ARCAT, Inc. - All rights reserved*

\*\* NOTE TO SPECIFIER \*\* Primacoustic (a division of Radial Engineering Ltd.); acoustic panels, T-bar ceiling tiles, clouds.  
This section is based on the products of Primacoustic (a division of Radial Engineering Ltd.), which is located at:  
1845 Kingsway Ave. Unit 1165  
Port Coquitlam, BC, Canada V3C 1S9  
Tel: 604-942-1001  
Fax: 604-942-1010  
Email:[request info (BlakeB@primacoustic.com)](https://admin.arcat.com/users.pl?action=UserEmail&company=Primacoustic+(a+division+of+Radial+Engineering+Ltd.)&coid=53699&rep=&fax=604-942-1010&message=RE:%20Spec%20Question%20(09800ptc):%20%20&mf=)  
Web:<https://www.primacoustic.com>  
[[Click Here](https://www.arcat.com/arcatcos/cos53/arc53699.html)] for additional information.  
Primacoustic is a manufacturer of acoustic materials of all types. With over 30 years' experience in studio and live sound and 15 years in acoustics, we have amassed a tremendous resource in the form of knowledge that is interspersed throughout this web site. We firmly believe that by sharing knowledge, not only will you enjoy better results from our products, you will pass along your learning to others.

1. GENERAL
   1. SECTION INCLUDES

\*\* NOTE TO SPECIFIER \*\* Delete items below not required for project.

* + 1. Installation Hardware - Broadway Impalers
  1. RELATED SECTIONS

\*\* NOTE TO SPECIFIER \*\* Delete any sections below not relevant to this project; add others as required.

* + 1. Section 09 51 00 - Acoustical Ceilings.
  1. REFERENCES

\*\* NOTE TO SPECIFIER \*\* Delete references from the list below that are not actually required by the text of the edited section.

* + 1. ASTM International (ASTM):
       1. ASTM E84.
       2. Canada: CA Technical Bulletin 117-2013 Section 1.
    2. California Building Code.
       1. CAL117 California fire retardant test.
    3. Underwriters Laboratories Canada (ULc):
       1. ULc-S102-03 Class A/1.
  1. SUBMITTALS
     1. Submit under provisions of Section 01 30 00 - Administrative Requirements.
     2. Product Data:
        1. Manufacturer's data sheets on each product to be used.
        2. Preparation instructions and recommendations.
        3. Storage and handling requirements and recommendations.
        4. Typical installation methods.

\*\* NOTE TO SPECIFIER \*\* Delete if not applicable to product type.

* + 1. Verification Samples: Two representative units of each type, size, pattern, and color.
    2. Shop Drawings: Include details of materials, construction, and finish. Include relationship with adjacent construction.
  1. QUALITY ASSURANCE
     1. Manufacturer Qualifications: Company specializing in manufacturing products specified in this section with a minimum five years documented experience.
     2. Installer Qualifications: Company specializing in performing Work of this section with minimum two years documented experience with projects of similar scope and complexity.
     3. Source Limitations: Provide each type of product from a single manufacturing source to ensure uniformity.

\*\* NOTE TO SPECIFIER \*\* Include mock-up if the project size or quality warrant the expense. The following is one example of how a mock-up on might be specified. When deciding on the extent of the mock-up, consider all the major different types of work on the project.

* + 1. Mock-Up: Construct a mock-up with actual materials in sufficient time for Architect's review and to not delay construction progress. Locate mock-up as acceptable to Architect and provide temporary foundations and support.
       1. Intent of mock-up is to demonstrate quality of workmanship and visual appearance.
       2. If mock-up is not acceptable, rebuild mock-up until satisfactory results are achieved.
       3. Retain mock-up during construction as a standard for comparison with completed work.
       4. Do not alter or remove mock-up until work is completed or removal is authorized.
  1. PRE-INSTALLATION CONFERENCE
     1. Convene a conference approximately two weeks before scheduled commencement of the Work. Attendees shall include Architect, Contractor and trades involved. Agenda shall include schedule, responsibilities, critical path items and approvals.
  2. DELIVERY, STORAGE, AND HANDLING
     1. Store and handle in strict compliance with manufacturer's written instructions and recommendations.
     2. Protect from damage due to weather, excessive temperature, and construction operations.
  3. PROJECT CONDITIONS
     1. Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's recommended limits.
  4. WARRANTY
     1. Manufacturer's standard limited warranty unless indicated otherwise.

1. PRODUCTS
   1. MANUFACTURERS
      1. Acceptable Manufacturer: Primacoustic (a division of Radial Engineering Ltd.), which is located at: 1845 Kingsway Ave. Unit 1165; Port Coquitlam, BC, Canada V3C 1S9; Tel: 604-942-1001; Fax: 604-942-1010; Email:[request info (BlakeB@primacoustic.com)](https://admin.arcat.com/users.pl?action=UserEmail&company=Primacoustic+(a+division+of+Radial+Engineering+Ltd.)&coid=53699&rep=&fax=604-942-1010&message=RE:%20Spec%20Question%20(09800ptc):%20%20&mf=); Web:<https://www.primacoustic.com>

\*\* NOTE TO SPECIFIER \*\* Delete one of the following two paragraphs; coordinate with requirements of Division 1 section on product options and substitutions.

* + 1. Substitutions: Not permitted.
    2. Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
  1. INSTALLATION HARDWARE – BROADWAY IMPALERS

\*\* NOTE TO SPECIFIER \*\* Delete hardware options not required.

* + 1. Push-On Impaler: To mount Broadway glass wool panels onto walls. Allow installer to push panels straight onto Impaler clips. Impaler feature sharp protruding darts that penetrate the panel and secure it in place.
       1. Construction adhesive is usually at center of Impaler during mounting.
       2. Impalers are mounted using sheetrock anchors and screws.
       3. Dimensions: 3 x 4 inch (76 x 102 mm).
       4. Material 20 gauge galvanized steel.
       5. Attachment Points: 2. Use appropriate fastener for wall surface.
       6. Load Limit: 12 lbs (5.4 kg); dependent on wall fastener.
    2. Surface Impaler: To mount Broadway glass wool panels onto walls. Allow installer to pull panel down onto Impaler clip while allowing for some levelling adjustability after the panel is installed. Impaler features four sharp darts that penetrate the panel and secure it in place.
       1. Construction adhesive is usually at center of Impaler during mounting.
       2. Impalers are mounted using sheetrock anchors and screws.
       3. Dimensions: 3 x 4 inch (76 x 102 mm).
       4. Material 20 gauge galvanized steel.
       5. Attachment Points: 2. Use appropriate fastener for wall surface.
       6. Load Limit: 12 lbs. (5.4 kg.); dependent on wall fastener.
    3. Offset Impaler: To mount Broadway glass wool acoustic panels onto wall surfaces while creating an air cavity behind the panel to increase bass absorption.
       1. U-shaped design that holds the panel from the wall surface by 3.5 inches (89 mm) making it easy to align with typical 2 x 4 inch (51 x 102 mm) studs.
       2. Panels held in place using a series of sharp protruding darts that penetrate the panel to secure it during installation.
       3. Construction adhesive is usually at center of Impaler during mounting.
       4. Impalers are mounted using sheetrock anchors and screws.
       5. Material: 20 gauge galvanized steel
       6. Dimensions: 3 x 5 inch (76 x 127 mm).
          1. Offset: 3.5 inch (89 mm) from wall surface.
       7. Attachment Points: 4. Use appropriate fastener for wall surface.
       8. Load Limit: 12 lbs (5.4 kg); dependent on wall fastener.
    4. Corner Impaler: To mount Broadway glass wool acoustic panels into corners to create bass traps. Features a 45 degree angle design that positions a panel across a typical 90 degree corner without causing serious defacement of the wall surface.
       1. Panel are held in place using a series of sharp protruding darts that penetrate the panel to secure it during installation.
       2. To ensure panels do not get dislodged after installation, a dab of construction adhesive may be applied to the impaler darts during the mounting process adding a higher level of security and reducing opportunity for tampering. Impalers are installed using typical sheetrock anchors and screws.
       3. Construction adhesive is usually at center of Impaler during mounting.
       4. Impalers are mounted using sheetrock anchors and screws.
       5. Material: 20 gauge galvanized steel.
       6. Dimensions: 3 x 5 inch (76 x 127 mm).
          1. Corner: 45 degree angle for 90 degree corners.
       7. Attachment Points: 4. Use appropriate fastener for wall surface.
       8. Load Limit: 12 lbs (5.4 kg); dependent on wall fastener.

1. EXECUTION
   1. EXAMINATION
      1. Do not begin installation until substrates have been properly constructed and prepared.
      2. If substrate preparation is the responsibility of another installer, notify Architect in writing of unsatisfactory preparation before proceeding.
   2. PREPARATION
      1. Clean surfaces thoroughly prior to installation.
      2. Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
   3. INSTALLATION
      1. Install in accordance with manufacturer's instructions, approved submittals, and in proper relationship with adjacent construction.
   4. FIELD QUALITY CONTROL
      1. Field Inspection: Coordinate field inspection in accordance with appropriate sections in Division 01.

\*\* NOTE TO SPECIFIER \*\* Include if manufacturer provides field quality control with onsite personnel for instruction or supervision of product installation, application, erection, or construction. Delete if not required.

* + 1. Manufacturer's Services: Coordinate manufacturer's services in accordance with appropriate sections in Division 01.
  1. CLEANING AND PROTECTION
     1. Clean products in accordance with the manufacturers recommendations.
     2. Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION